**Cond (Condition) Column Codes-Definitions**

AR - Removed (removed but not repaired or overhauled)

US - removed but unserviceable

RP – same as above

SV or SRV - serviceable (good, just not tested)

OH - overhauled (ready to be installed)

NE - brand new

NS - new surplus (never used, but not traced to OEM)

BER - beyond economic repair or less to buy new